

                                                                                         
	Contract Name 
	

	Contract Number
	

	Commencement Date
	

	Signals Contractor
	

	Civil Contractor
	

	CONTROLLER
	Y/N /NA                       Comments

	Make & Type:
	Make:                          VC:                        ELV: Yes/No

	Signal Group Size / No. of
		8
	
	12
	
	16
	
	24
	
	32
	
	
	




	Detector Card Size / No. of
		8
	
	12
	
	16
	
	24
	
	32
	
	
	




	Communication Type/Number
	

	ICP Number
	

	Det Card Operation Check
	
	

	Labels (Gland Plate & Cable looms)
	
	

	Labels (RCD’s & Streetlights)
	
	

	Numbering (Signal groups, det card)
	
	

	Cable Glands Sealed
	
	

	Spare Sockets Working
	
	

	Controller Cabinet Earthed
	
	

	Wiring Tidy
	
	

	Draw Cables Installed
	
	

	Vertical & Secure
	
	

	Door Seals and Locks
	
	

	Sticker(s)
	
	

	POLES
	Y/N /NA                       Comments

	Correct Location
	
	

	Concrete Collar (500mm)
	
	

	Cables Terminated OK
	
	

	Painted / Powder Coating
	
	

	Sockets Installed
	
	

	Fold Down Poles Work
	
	

	Mast arm outreach length
	
	

	UMB & Finial Cap
	
	

	Ethernet & draw cables
	
	

	Pole Numbers Installed
	
	

	LANTERNS
	Y/N /NA                       Comments

	Attached Securely
	
	

	Aligned Correctly
	
	

	Correct Heights
	
	

	Correct Aspects
	
	

	Correct Louvers / Visors
	
	

	Ped Lanterns correct
	
	

	PED/CYCLE CROSSINGS
	Y/N /NA                       Comments

	Push Buttons:

	Install Correct Height (1.1m)
	
	

	Dynamic Audio Working
	
	

	Tactile Vibration Working
	
	

	Arrow Aligned to Crossing
	
	

	PB Light Indicator (If Fitted)
	
	

	Ped Detectors (if provided):

	Detectors Installed OK
	
	

	Instruction Labels Installed
	
	

	DETECTOR LOOPS
	Y/N /NA                       Comments

	Loops Positioned Correctly
	
	

	Sealant Installed Cleanly
	
	

	KJB 100mm concrete surround
	
	

	KJB drainage material
	
	

	Loop Joins with gel connectors
	
	

	>1.8m Slack in Contr Base 
	
	

	>0.5m Slack in KJB
	
	

	CIVIL WORKS
	Y/N /NA                       Comments

	Correct Ducting as per Specs
	
	

	Chambers Level with Surface
	
	

	Duct Connections in Chamber
	
	

	1m Cable Slack in Chambers
	
	

	Duct Connections to Poles
	
	

	Road Surface Condition
	
	

	Pathway Surface Condition
	
	

	Pram Ramps Installed
	
	

	Warning Tactiles Aligned
	
	

	Directional Pavers across paths
	
	

	Road Markings Correct
	
	

	Drainage, Esp at Crossings.
	
	

	Grass Berms Restored
	
	

	Sweeping Completed
	
	

	Correct Signage Installed
	
	

	Temp Advance Warnings
	
	

	DOCUMENTATION
	Y/N /NA                       Comments

	In Controller (Laminated)

	C & I
	
	

	Impendence test report (non ELV)
	
	

	Intersection As-Built Drawing
	
	

	AGD Instruction Sheets
	
	

	Controller Information Sheets
	
	

	Log Book
	
	

	OPERATIONS
	Y/N /NA                       Comments

	E-Prom Labelled (check sum)
	
	

	Lamps Off, Controller Ops
	
	

	SCATS Communication (24hrs)
	
	

	Check Fault Log, Clear.
	
	

	Full Start Up:

	Flash Test Each SG
	
	

	Flashing Ambers Working
	
	

	Check All Red (SPT=10s)
	
	

	Revision On Correct Phases
	
	

	All Default Phases Call
	
	

	Other Phases Call
	
	

	Ped Protection OK
	
	

	Ped detector zones (if installed)
	
	

	Special logic OK (check CIS) e.g.
· Filtering 
· Hurry call
· Separated ped input buttons 
· On-crossing detection
· Ped reintroduction/WFG
	
	

	OTHER
	Y/N /NA                       Comments

	Camera connected & Working
	
	

	Cycle loop sensitivity (e.g. 0.05)
	
	

	Above Ground Detectors ok
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	Intersection Name
	Browns Rd Ped

	Number
	
	
	Date
	23/07/2005

	
	
	
	Audit #
	1
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SITE ACCEPTANCE TEST (SAT) – NEW SITE
	INTERSECTION NAME
	

	NUMBER
	
	DATE
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REMEDIAL LIST
	No
	Fault:
	Action:
	Completed Date:

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	Faults that need to be addressed before site can be switched on:

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

		Approved for switch on?    YES  /  NO
If yes, has the site been commissioned?    YES  /  NO


	Traffic Signal Representative:                                                                   


	Sign:                                                                                       Date:


	Signal Contractor:    


	Sign:                                                                                       Date:


	HAND OVER TO RCA OPERATIONS WHEN SIGNED ABOVE
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