




	Signals Contractor
	

	Civil Contractor
	

	NEW CONTROLLER?
	Circle:  NO or YES

	Make & Type:
	Make:                          VC:                        ELV: Yes/No

	Signal Group Size / No. of
		8
	
	12
	
	16
	
	32
	
	




	Detector Card Size / No. of
		8
	
	12
	
	16
	
	32
	
	




	Labels & Numbering
	
	

	Cabinet Earthed
	
	

	Wiring complete and tidy
	
	

	Stickers
	
	

	NEW POLES or LANTERNS?
	Circle NO or YES. If yes, enter pole no’s:

	Correct Location
	
	

	Collar, coating, Finial Cap
	
	

	Pole Numbers Installed
	
	

	Lanterns have correct aspects
	
	

	Lantern alignment and visors
	
	

	Push buttons correct height
	
	

	Push button sound, indicator light
	
	

	NEW DETECTORS?
	Circle NO or YES. If yes, enter det no’s: 

	Loops Positioned Correctly
	
	

	Sealant Installed Cleanly
	
	

	KJB surround, slack, wiring joints
	
	

	Check working on detector board
	
	

	NEW CHAMBERS?
	Circle NO or YES

	Correct Ducting as per design
	
	

	Chambers Level, Duct connections
	
	

	1m Cable Slack
	
	

	CIVIL WORKS?
	Tick or N/A for each item

	Road & Path Surface Condition
	
	

	Pram Ramps incl drainage
	
	

	Tactile Pavers
	
	

	Grass Berms
	
	

	Signage
	
	

	NEW SOFTWARE?
	Circle NO or YES

	Flashing Amber, Phases Call
	
	

	Ped protection OK
	
	

	Operation OK incl special logic
	
	

	OTHER
	Tick or N/A for each item

	SCATS comms
	
	

	Camera connected & Working
	
	

	New documentation (As-built, CIS)
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	Intersection Name
	Browns Rd Ped

	Number
	
	
	Date
	23/07/2005

	
	
	
	Audit #
	1



1


SITE ACCEPTANCE TEST (SAT) – UPGRADE WORKS
	INTERSECTION NAME
	

	NUMBER
	
	DATE
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	OPERATION TESTING
	MUST BE COMPLETED IF ANY SIGNAL GROUP WIRING HAS CHANGED, BEFORE SWITCH ON

	Testing required?
	Circle NO or YES

	Test
	When to test
	Complete?

	Flash test each Signal Group
	Preferred test.
Must be safe to do so, e.g. roads are quiet/night
or site is under traffic management control
	

	Watch Signal Group operation
	If not safe to do a flash test.
Each signal group must be observed/checked.
Diamond signal groups (e.g. those in a D1/D2 phase or G1/G2 phase) must have each of those phases locked on via SCATS or detector board.
For example: Lock on all peds and the TH+RT detectors for the approach and check the correct signal groups run in each diamond phase, i.e. it should be SG1+3 together, SG2+4 together, etc.
	


 

REMEDIAL LIST
	No
	Fault:
	Action:
	Completed Date:

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

		Approved for switch on?    YES  /  NO
If yes, has the site been commissioned?    YES  /  NO


	Traffic Signal Representative:                                                                   


	Sign:                                                                                       Date:


	Signal Contractor:    


	Sign:                                                                                       Date:


	HAND OVER TO RCA OPERATIONS WHEN SIGNED ABOVE
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